8 BIT ADDITION

Program:

LDA 8500

MOV B,A

LDA 8501

ADD B

STA 8502

RST 1

OUTPUT: